|  |  |
| --- | --- |
| **Name:** |  |
| **Date:** |  |
| **TASK:** | **Chainsaw – 2 Stroke** | **Stage 1 of 2 stages in task** |
| TA: | Start  |
| **Name of Assessor:** |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| A Skill level of**...A...B...C...D...E...**Indicate level using underpinning work skill guide**Steps requiring skill level : List by step number**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |

**Office use only** |

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Assistance coding:**0=no assistance/fully independent1=indirect verbal prompts/instructions2=gestural prompts3=direct verbal prompts/instructions4=model style prompting5=physical prompting MINIMAL6=physical prompting FULL assistance7=not complaint/failed taskN/A=not applicable  | OBSERVATION DATES  | Associated: * Safe Work Procedure
* Safety Data Sheet

OHS requirements* Safety Glasses
* Gloves - tech/riggers
* Ear muffs
* Steel capped boots
* Work clothing
* Sun protection
 |
| 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | **Staff initials**: |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | STEPS  | ASSISTANCE REQURED |
| **1** | Use of OHS requirements |  |  |  |  |  |  |  |  |  |  |  |  |  | SUPERVISOR:* Pre – safety checks
* Worker supervision is required when refuelling
 |
| **2** | Check work area is safe before starting chainsaw |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **3** | Activate chain brake by pushing it forward |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **4** | Remove bar cover before starting  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **5** | Check bar oil |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **6** | Press decompression valve and /or primer bulb to assist starting if required |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **7** | Set control lever to choke/cold start. Press throttle trigger then master control lever all the way down |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **8** | To start lay on flat surface not letting the blade touch the ground |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **9** | Place left hand on handlebar and right hand on starter rope. Push right foot toecap into rear handle to stabilise chainsaw |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **10** | Slowly pull the starter rope with right hand until you feel resistance. Then pull rope hard several times until engine fires briefly. Pull it upward in vertical manner |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **11** | Move master control lever up one notch to open the choke |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **12** | Pull starter rope again till engine fires again |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **13** | As soon as engine has fired and is running, touch throttle trigger briefly, master control moves to idle setting |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **14** | Slowly lift chainsaw without touching throttle trigger |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **15** | Release chain break keeping hold of handlebar with left hand until you hear a click |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

**Comments:**

|  |
| --- |
|  |